RFID SCANNER MOTE:
AutoScanRFID goes onto the motes.

information for the hardware.
http://seattleweb.intel-research.net/projects/guide/projects/iglove/RFIDglove.htm



COMPACT FLASH MOTE:
The TOSBase goes on the compact flash mote.  Compile the code with the command:

make install mica2

then take the binary generated and load it onto the Compact Flash Mote.