The serial forwarder needs to be compiled for ARM platform using arm-linux-gcc.
Making "asf" should produce the executable proram.

It can then be executed like so:
	asf <port> <device> <baud>

e.g.
	asf 4444 /dev/tts/3 57600

We use this command to forward packets from a mote embedded in a compact flash card.